## **CP30-H0727-N**

**Technical Specifications**

|  |  |
| --- | --- |
| Frequency Range | 698~2700MHz |
| Coupling Level | 30dB |
| Coupling Uniformity | ±1.5dB |
| Insertion Loss | ≤0.3dB |
| Directivity | ≥20dB |
| VSWR | ≤1.3 |
| Impedance | 50 Ω |
| Power Handling | 200W |
| PIM3 | ≤-150dBc@2\*20W |
| Connector | N Female |
| Operating Temperature | -25~+65 °C |
| Relative Humidity | 0~95 % |
| Application | Indoor or Outdoor (IP65) |
| Dimensions | 160x62x17.6 mm |
| Ports | 1 input ports + 2 output ports |
| Weight | ≤0.5kg |
| Inner Contact Plating | Silver |
| Outer Contact Plating | Silver |

**Drawing**

